DICOM PS3.3 2017e - Information Object Definitions

A.34.5.4.7 Waveform Sample Interpretation
Prev | A.34.5.4 Ambulatory ECG IOD Content Constraints | Next

##### A.34.5.4.7 Waveform Sample Interpretation

The value of Waveform Sample Interpretation (5400,1006) in each Waveform Sequence Item shall be SB or SS.

Prev | Up | Next
A.34.5.4.6 Channel Source | Home | A.34.6 Hemodynamic IOD

DICOM PS3.3 2017e - Information Object Definitions