DICOM PS3.4 2017e - Service Class Specifications

DD.3.2.3 N-ACTION
Prev | DD.3.2 DIMSE Service Group | Next

#### DD.3.2.3 N-ACTION

The N-ACTION is used to initiate parameter verification of an instance of the applicable Machine Verification SOP Class.

##### DD.3.2.3.1 Attributes

The action types of the N-ACTION are defined as shown in Table DD.3.2.3-1.

Table DD.3.2.3-1. Action Event Information

Action Type Name | Action Type ID | Attribute Name | Tag | Usage SCU/SCP
--- | --- | --- | --- | ---
Request Beam Verification | 1 | None | - | -

Prev | Up | Next
DD.3.2.2.4 Behavior | Home | DD.3.2.3.2 Status

DICOM PS3.4 2017e - Service Class Specifications