DICOM PS3.16 2017e - Content Mapping Resource

TID 3715 ECG Measurement Source
Prev | ECG Report Templates | Next

### TID 3715 ECG Measurement Source

The ECG Measurement Source Template provides a structure for identifying the particular cardiac cycle, or beat, in an analyzed ECG waveform used for the measurement group for which this Template provides Observation Context. The cardiac cycle is identified by beat number, and optionally by specific temporal coordinates within a DICOM ECG Waveform SOP Instance.

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 3715. ECG Measurement Source

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | TEXT | EV (122149, DCM, "Beat Number") | 1 | U |  | Up to three numeric characters
2 |  |  | CODE | EV (G-C036, SRT, "Measurement Method") | 1 | U |  | DCID 3676 “Lead Measurement Technique”
3 |  |  | TCOORD | EV (121112, DCM, "Source of Measurement") | 1 | U |  |
4 | > | SELECTED FROM | WAVEFORM |  | 1 | U |  |

Content Item Descriptions

Row 1 | Beat Number is specified as a numeric text string, and shall be treated as the ordinal of the beat (cardiac cycle) within the waveform acquisition for this lead that was analyzed for the measurements in this container (i.e., "1" for the first beat, "2" for the second, etc.). If absent, the measurements may have been made by a technique across multiple cycles as specified in Row 2 Measurement Method.
Rows 3 and 4 | Source of measurement identify the specific channel and time period within a DICOM ECG Waveform SOP Instance that was analyzed for the measurements in this container.

Prev | Up | Next
TID 3714 ECG Lead Measurements | Home | TID 3717 ECG Qualitative Analysis

DICOM PS3.16 2017e - Content Mapping Resource