DICOM PS3.4 2017e - Service Class Specifications

GG.3 SOP Classes
Prev | GG Non-Patient Object Storage Service Class | Next

## GG.3 SOP Classes

The application-level services addressed by the Non-Patient Object Storage Service Class definition are specified in the SOP Classes specified in Table GG.3-1.

Table GG.3-1. Standard SOP Classes

SOP Class Name | SOP Class UID | IOD Specification (defined in PS3.3)
--- | --- | ---
Hanging Protocol Storage | 1.2.840.10008.5.1.4.38.1 | Hanging Protocol IOD
Color Palette Storage | 1.2.840.10008.5.1.4.39.1 | Color Palette IOD
Generic Implant Template Storage | 1.2.840.10008.5.1.4.43.1 | Generic Implant Template IOD
Implant Assembly Template Storage | 1.2.840.10008.5.1.4.44.1 | Implant Assembly Template IOD
Implant Template Group Storage | 1.2.840.10008.5.1.4.45.1 | Implant Template Group IOD
CT Defined Procedure Protocol Storage | 1.2.840.10008.5.1.4.1.1.200.1 | CT Defined Procedure Protocol IOD
Protocol Approval Storage | 1.2.840.10008.5.1.4.1.1.200.3 | Protocol Approval IOD

Prev | Up | Next
GG.2 Association Negotiation | Home | GG.4 Behavior

DICOM PS3.4 2017e - Service Class Specifications