DICOM PS3.3 2017e - Information Object Definitions

A.8.2.4 Multi-frame Single Bit SC Image IOD Content Constraints
Prev | A.8.2 Multi-frame Single Bit Secondary Capture Image IOD | Next

#### A.8.2.4 Multi-frame Single Bit SC Image IOD Content Constraints

In the Image Pixel Module, the following constraints apply:

- Samples per Pixel (0028,0002) shall be 1

- Photometric Interpretation (0028,0004) shall be MONOCHROME2

- Bits Allocated (0028,0100) shall be 1

- Bits Stored (0028,0101) shall be 1

- High Bit (0028,0102) shall be 0

- Pixel Representation (0028,0103) shall be 0

- Planar Configuration (0028,0006) shall not be present

### Note

As a consequence of these attribute values, single bit pixels are packed eight to a byte as defined by the encoding rules in PS3.5.

The VOI LUT Module shall not be present.

The Overlay Plane Module shall not be present.

Prev | Up | Next
A.8.2.3 Multi-frame Single Bit SC Image IOD Module Table | Home | A.8.3 Multi-frame Grayscale Byte Secondary Capture Image IOD

DICOM PS3.3 2017e - Information Object Definitions