DICOM PS3.3 2017e - Information Object Definitions

A.18 RT Dose IOD
Prev | A Composite Information Object Definitions (Normative) | Next

## A.18 RT Dose IOD

### A.18.1 RT Dose IOD Description

The focus for this Radiotherapy Dose IOD (RT Dose IOD) is to address the requirements for transfer of dose distributions calculated by radiotherapy treatment planning systems. These distributions may be represented as 2D or 3D grids, as isodose curves, or as named or unnamed dose points scattered throughout the volume. This IOD may also contain dose-volume histogram data, single or multi-frame overlays and application-defined lookup tables. This IOD does not provide for definition of doses in beam or other coordinate systems. The application is responsible for transforming data in other, non-patient based coordinate systems to the patient based coordinate system described in Section C.7.6.2.1.1.

Prev | Up | Next
A.17.3 RT Image IOD Module Table | Home | A.18.2 RT Dose IOD Entity-Relationship Model

DICOM PS3.3 2017e - Information Object Definitions