DICOM PS3.3 2018a - Information Object Definitions

C.12.3 Frame Extraction Module
Prev | C.12 General Modules | Next

### C.12.3 Frame Extraction Module

Table C.12-9 defines the Attributes that describe the frames extracted if the SOP Instance was created in response to a Frame-Level retrieve request.

Table C.12-9. Frame Extraction Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Frame Extraction Sequence | (0008,1164) | 1 | Sequence containing details of how this SOP Instance was extracted from a source multi-frame SOP Instance. If this instance was created from an instance that contains a Frame Extraction Sequence, then this sequence shall contain all of the items from the parent's Frame Extraction Sequence and a new item that describes this extraction. One or more Items shall be included in this Sequence.
>Multi-frame Source SOP Instance UID | (0008,1167) | 1 | SOP Instance from which the frames of this instance are extracted.
>Simple Frame List | (0008,1161) | 1C | A list of Frames that were extracted in the form of a simple list. Required if object extraction is based on a Frame Level Retrieve using the Simple Frame List (0008,1161) attribute. See PS3.4 "Instance and Frame Level Retrieve SOP Classes"
>Calculated Frame List | (0008,1162) | 1C | A list of Frames that were extracted in the form of one or more triplets Required if object extraction is based on a Frame Level Retrieve using the Calculated Frame List (0008,1162) attribute. See PS3.4 "Instance and Frame Level Retrieve SOP Classes"
>Time Range | (0008,1163) | 1C | The start and end times of the frames that were extracted. Required if object extraction is based on a Frame Level Retrieve using Time Range (0008,1163). See PS3.4 "Instance and Frame Level Retrieve SOP Classes"

Prev | Up | Next
C.12.2 Common Instance Reference Module | Home | C.12.4 General Reference Module

DICOM PS3.3 2018a - Information Object Definitions