DICOM PS3.17 2018a - Explanatory Information

XXX.3.7.3 Encoding Details
Prev | XXX.3.7 Ultrasound Color Flow MPR | Next

#### XXX.3.7.3 Encoding Details

##### XXX.3.7.3.1 Volumetric Presentation State Relationship Module Recommendations

Table XXX.3.7-1. Volumetric Presentation State Relationship Module Recommendations

Attribute Name | Tag | Comment
--- | --- | ---
Volumetric Presentation State Input Sequence | (0070,1201) | Two items are this sequence referencing one volume for each data type
>ITEM 1
>Volumetric Presentation Input Number | (0070,1207) | Set to 1
>Presentation Input Type | (0070,1202) | Set to "VOLUME".
>Referenced Image Sequence | (0008,1140) | Sequence of frames with Data Type (0018,9808) value of TISSUE_INTENSITY
>>Table 10-3 “Image SOP Instance Reference Macro Attributes” in PS3.3
>Crop | (0070,1204) | Set to "NO".
>ITEM 2
>Volumetric Presentation Input Number | (0070,1207) | Set to 2
>Presentation Input Type | (0070,1202) | Set to "VOLUME".
>Referenced Image Sequence | (0008,1140) | Sequence of frames with Data Type (0018,9808) value of FLOW_VELOCITY
>>Table 10-3 “Image SOP Instance Reference Macro Attributes” in PS3.3
>Crop | (0070,1204) | Set to "NO".

Prev | Up | Next
XXX.3.7.2 Encoding Outline | Home | XXX.3.7.3.2 Presentation View Description Module Recommendations

DICOM PS3.17 2018a - Explanatory Information