DICOM PS3.16 2018a - Content Mapping Resource

TID 3515 Cardiac Output Measurement by Indicator Dilution
Prev | Hemodynamics Report Templates | Next

### TID 3515 Cardiac Output Measurement by Indicator Dilution

The Cardiac Output Measurement by Indicator Dilution Template consists of a CONTAINER containing the measurement and significant parameters of the technical method. If the measurement is based on a DICOM Hemodynamic Waveform SOP Instance, that object may also be referenced.

### Note

Fick Cardiac Output is encoded in TID 3560 “Derived Hemodynamic Measurements”.

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 3515. Cardiac Output Measurement By Indicator Dilution

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (P2-34201, SRT, "Cardiac Output measurement") | 1 | M |  |
2 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = EV (8737-9, LN, "Cardiac Output by Indicator Dilution") $Units = EV (l/min, UCUM, "l/min") $Method = DCID 3628 “Cardiac Output Methods” $WavePurpose = DT (121112, DCM, "Source of Measurement")
3 | > | HAS ACQ CONTEXT | NUM | EV (122319, DCM, "Catheter Size") | 1 | MC | IFF Row 2 indicates a thermal method | UNITS = DCID 3510 “Catheter Size Units”
4 | > | HAS ACQ CONTEXT | NUM | EV (122320, DCM, "Injectate Temperature") | 1 | MC | IFF Row 2 indicates a thermal method | UNITS = EV (Cel, UCUM, "C")
5 | > | HAS ACQ CONTEXT | NUM | EV (122321, DCM, "Injectate Volume") | 1 | M |  | UNITS = DT (ml, UCUM, "ml")
6 | > | HAS ACQ CONTEXT | NUM | EV (122322, DCM, "Calibration Factor") | 1 | M |  | UNITS = DT (1, UCUM, "no units")

Prev | Up | Next
TID 3510 Vital Signs | Home | TID 3516 Blood Lab Measurements

DICOM PS3.16 2018a - Content Mapping Resource