DICOM PS3.17 2018a - Explanatory Information

HHH Transition from WADO to RESTful Services (Informative)
Prev |  | Next

# HHH Transition from WADO to RESTful Services (Informative)

This annex discusses the design considerations that went into the definition of the WADO extension to Web and REST services.

## HHH.1 Request and Response Parameters

### HHH.1.1 Request Parameters

The WADO-RS and STOW-RS requests have no parameters because data is requested through well defined URLs and content negotiation through HTTP headers.

Table HHH.1-1. Summary of DICOM/Rendered URI Based WADO Parameters

Parameter | Allowed for | Requirement in Request
--- | --- | ---
requestType | DICOM & Rendered | Required
studyUID | DICOM & Rendered | Required
seriesUID | DICOM & Rendered | Required
objectUID | DICOM & Rendered | Required
contentType | DICOM & Rendered | Optional
charset | DICOM & Rendered | Optional
anonymize | DICOM | Optional
annotation | Rendered | Optional
Rows, columns | Rendered | Optional
region | Rendered | Optional
windowCenter, windowWidth | Rendered | Optional
imageQuality | DICOM & Rendered | Optional
presentationUID | Rendered | Optional
presentationSeriesUID | Rendered | Optional
transferSyntax | DICOM | Optional
frameNumber | DICOM & Rendered | Optional

### HHH.1.2 Response Parameters

#### HHH.1.2.1 URI WADO-URI

In the URI based WADO, the response is the single payload returned in the HTTP Get response. It may be the DICOM object in a DICOM format or in a rendered format.

#### HHH.1.2.2 Retired

See PS3.17-2017b.

#### HHH.1.2.3 WADO-RS

The WADO-RS Service is a transport service, as opposed to a rendering service, which provides resources that enable machine to machine transfers of binary instances, pixel data, bulk data, and metadata. These services are not primarily intended to be directly displayable in a browser.

In the REST Services implementation:

- For the "DICOM Requester", one or more multipart/related parts are returned containing PS3.10 binary DICOM instances of a Study, Series, or a single Instance.

- For the "Frame Pixel Data Requester", one or more multipart/related parts are returned containing the pixel data of a multi-frame SOP Instance.

- For the "Bulk Data Requester", one or more multipart/related parts are returned containing the bulk data of a Study, Series or SOP Instance.

- For the "Metadata Requester", an item is returned containing the XML encoded metadata selected from the retrieved objects header as described in the Native DICOM Model defined in PS3.19.

#### HHH.1.2.4 STOW-RS

The STOW-RS Service provides the ability to STore Over the Web using RESTful Services (i.e., HTTP based functionality equivalent to C-Store).

- For the "DICOM Creator", one or more multipart/related parts are stored (posted to a STOW-RS Service) containing one or more DICOM Composite SOP Instances.

- For the "Metadata and Bulk Data Creator", one or more multipart/related parts are stored (posted to a STOW-RS Service) containing the XML encoded metadata defined in PS3.19 and one or more parts containing the bulk data of a Study, Series or SOP Instance.

Prev |  | Next
GGG.3.3 Gift Subscriptions | Home | HHH.2 Web Services Implementation

DICOM PS3.17 2018a - Explanatory Information