DICOM PS3.3 2018a - Information Object Definitions

A.76.4.3 ICC Profile Module
Prev | A.76.4 Wide Field Ophthalmic Photography Stereographic Projection Image IOD Content Constraints | Next

#### A.76.4.3 ICC Profile Module

The ICC Profile Module shall be present for color images. If the color space to be used is not calibrated (i.e., a device-specific ICC Input Profile is not available), then an ICC Input Profile specifying a well-known space (such as sRGB) may be specified.

Prev | Up | Next
A.76.4.2 Contrast/Bolus Agent Sequence | Home | A.77 Wide Field Ophthalmic Photography 3D Coordinates Image IOD

DICOM PS3.3 2018a - Information Object Definitions