DICOM PS3.4 2018a - Service Class Specifications

EE.2.2 DIMSE Service Group
Prev | EE.2 Display System SOP Class | Next

### EE.2.2 DIMSE Service Group

The DIMSE Service shown in Table EE.2.2-1 is applicable to the Display System IOD under the Display System SOP Class.

Table EE.2.2-1. DIMSE Service Group - Display System

DIMSE Service Element | Usage SCU/SCP
--- | ---
N-GET | M/M

This section describes the behavior of the DIMSE services that are specific for this IOD. The general behavior of the DIMSE services is specified in PS3.7.

#### EE.2.2.1 N-GET

N-GET is used to retrieve information from an instance of the Display System SOP class.

##### EE.2.2.1.1 Attributes

###### EE.2.2.1.1.1 Display Subsystem Macros

To reduce the size and complexity of EE.2.2.1-2, a macro notation is used.

Table EE.2.2.1-1. Table Result Context Macro

Attribute Name | Tag | Usage SCU/SCP
--- | --- | ---
Performed Procedure Step Start DateTime | (0040,4050) | -/1
Performed Procedure Step End DateTime | (0040,4051) | -/1
Actual Human Performer Sequence | (0040,4035) | 3/2
>Human Performer Code Sequence | (0040,4009) | -/1C (Required if Human Performer's Name (0040,4037) is not present.)
>>Include Table CC.2.5-2a “UPS Code Sequence Macro”
>Human Performer's Name | (0040,4037) | -/1C (Required if Human Performer Code Sequence (0040,4009) is not present.)
>Human Performer's Organization | (0040,4036) | -/2
Measurement Equipment Sequence | (0028,7012) | 3/2
>Measurement Functions | (0028,7013) | -/1
>Measured Characteristics | (0028,7026) | -/1
>Measurement Equipment Type | (0028,7014) | -/1
>Manufacturer | (0008,0070) | -/1
>Manufacturer's Model Name | (0008,1090) | -/1
>Device Serial Number | (0018,1000) | -/2
>DateTime of Last Calibration | (0018,1202) | -/2

###### EE.2.2.1.1.2 Display System N-GET Attribute Requirements

The attributes that may be retrieved are shown in Table EE.2.2.1-2.

Table EE.2.2.1-2. Display System N-GET Attributes

Attribute Name | Tag | Usage SCU/SCP
--- | --- | ---
Specific Character Set | (0008,0005) | -/1C (Required if an extended or replacement character set is used)
Display System Module
Manufacturer | (0008,0070) | 3/1
Institution Name | (0008,0080) | 3/1
Institution Address | (0008,0081) | 3/1
Device Serial Number | (0018,1000) | 3/1
Station Name | (0008,1010) | 3/2
Institutional Department Name | (0008,1040) | 3/2
Manufacturer's Model Name | (0008,1090) | 3/1
Equipment Administrator Sequence | (0028,7000) | 3/2
>Person Name | (0040,A123) | -/2
>Person Identification Code Sequence | (0040,1101) | -/1
>>Include Table CC.2.5-2a “UPS Code Sequence Macro”
>Person's Address | (0040,1102) | -/3
>Person's Telephone Numbers | (0040,1103) | -/3
>Institution Name | (0008,0080) | -/1C (Required if Institution Code Sequence (0008,0082) is not present. May be present otherwise.)
>Institution Address | (0008,0081) | -/3
>Institution Code Sequence | (0008,0082) | -/1C (Required if Institution Name (0008,0080) is not present.May be present otherwise.)
>>Include Table CC.2.5-2a “UPS Code Sequence Macro”
Number of Display Subsystems | (0028,7001) | 3/1
Display Subsystem Sequence | (0028,7023) | 3/1
>Display Subsystem ID | (0028,7003) | -/1
>Display Subsystem Name | (0028,7004) | -/2
>Display Subsystem Description | (0028,7005) | -/2
>Display Device Type Code Sequence | (0028,7022) | -/2
>>Include Table CC.2.5-2a “UPS Code Sequence Macro”
>Manufacturer | (0008,0070) | -/2
>Device Serial Number | (0018,1000) | -/2
>Manufacturer's Model Name | (0008,1090) | -/2
>System Status | (0028,7006) | -/1
>System Status Comment | (0028,7007) | -/2
>Display Subsystem Configuration Sequence | (0028,700A) | -/2
>>Configuration ID | (0028,700B) | -/1
>>Configuration Name | (0028,700C) | -/2
>>Configuration Description | (0028,700D) | -/2
>>Referenced Target Luminance Characteristics ID | (0028,700E) | -/2
>Current Configuration ID | (0028,7002) | -/2
>Measurement Equipment Sequence | (0028,7012) | -/2
>>Measurement Functions | (0028,7013) | -/1
>>Measured Characteristics | (0028,7026) | -/1
>>Measurement Equipment Type | (0028,7014) | -/1
>>Manufacturer | (0008,0070) | -/1
>>Manufacturer's Model Name | (0008,1090) | -/1
>>Device Serial Number | (0018,1000) | -/1
>>DateTime of Last Calibration | (0018,1202) | -/2
Target Luminance Characteristics Module
Target Luminance Characteristics Sequence | (0028,7008) | 2/1
>Luminance Characteristics ID | (0028,7009) | -/1
>Display Function Type | (0028,7019) | -/1
>Target Minimum Luminance | (0028,701D) | -/1
>Target Maximum Luminance | (0028,701E) | -/1
>Gamma Value | (0028,701A) | -/1C (Required if the value of Display Function Type (0028,7019) is GAMMA)
>Number of Luminance Points | (0028,701B) | -/1C (Required if the value of Display Function Type (0028,7019) is USER_DEFINED)
>Luminance Response Sequence | (0028,701C) | -/1C (Required if the value of Display Function Type (0028,7019) is USER_DEFINED)
>>DDL Value | (0028,7017) | -/1
>>Luminance Value | (0028,701F) | -/1
>Luminance Response Description | (0028,7020) | -/1C (Required if the value of Display Function Type (0028,7019) is USER_DEFINED. May be present otherwise.)
>CIExy White Point | (0028,7018) | -/3
>Reflected Ambient Light | (2010,0160) | -/3
>Ambient Light Value Source | (0028,7025) | -/1C (Required if Reflected Ambient Light (2010,0160) is present.)
QA Results Module
QA Results Sequence | (0028,700F) | 3/1
>Display Subsystem ID | (0028,7003) | -/1
>Display Subsystem QA Results Sequence | (0028,7010) | -/2
>>Configuration ID | (0028,700B) | -/1
>> Configuration QA Results Sequence | (0028,7011) | -/2
>>>Display Calibration Result Sequence | (0028,7016) | -/2
>>>>Include Table EE.2.2.1-1 “Table Result Context Macro”
>>>>Luminance Characteristics ID | (0028,7009) | -/1
>>>Visual Evaluation Result Sequence | (0028,7015) | -/2
>>>>Include Table EE.2.2.1-1 “Table Result Context Macro”
>>>>Visual Evaluation Test Sequence | (0028,7028) | -/1
>>>>>Test Result | (0028,7029) | -/1
>>>>>Test Result Comment | (0028,702A) | -/3
>>>>>Test Pattern Code Sequence | (0028,702C) | -/3
>>>>>>Include Table CC.2.5-2a “UPS Code Sequence Macro”
>>>>>Referenced Image Sequence | (0008,1140) | -/1C (Required if Test Pattern Code Sequence (0028,702C) is absent in this item.May be present otherwise.)
>>>>>>Referenced SOP Class UID | (0008,1150) | -/1
>>>>>>Referenced SOP Instance UID | (0008,1151) | -/1
>>>>>>Referenced Frame Number | (0008,1160) | -/1C (Required if the Referenced SOP Instance is a multi-frame image and the reference does not apply to all frames, and Referenced Segment Number (0062,000B) is not present.)
>>>>>>Referenced Segment Number | (0062,000B) | -/1C (Required if the Referenced SOP Instance is a Segmentation or Surface Segmentation and the reference does not apply to all segments and Referenced Frame Number (0008,1160) is not present.)
>>>>>>Test Image Validation | (0028,702B) | -/3
>>>>Visual Evaluation Method Code Sequence | (0028,702E) | -/1
>>>>>Include Table CC.2.5-2a “UPS Code Sequence Macro”
>>>Luminance Uniformity Result Sequence | (0028,7027) | -/2
>>>>Include Table EE.2.2.1-1 “Table Result Context Macro”
>>>>Number of Luminance Points | (0028,701B) | -/1
>>>>Measurement Pattern Code Sequence | (0028,702D) | -/1
>>>>>Include Table CC.2.5-2a “UPS Code Sequence Macro”
>>>>DDL Value | (0028,7017) | -/1
>>>>White Point Flag | (0028,7021) | -/1
>>>>Luminance Response Sequence | (0028,701C) | -/1
>>>>>Luminance Value | (0028,701F) | -/1
>>>>>CIExy White Point | (0028,7018) | -/1C (Required if the value of White Point Flag (0028,7021) is YES.)
>>>>Reflected Ambient Light | (2010,0160) | -/3
>>>>>Ambient Light Value Source | (0028,7025) | -/1C (Required if Reflected Ambient Light (2010,0160) is present.)
>>>Luminance Result Sequence | (0028,7024) | -/2
>>>>Include Table EE.2.2.1-1 “Table Result Context Macro”
>>>>Number of Luminance Points | (0028,701B) | -/1
>>>>Luminance Response Sequence | (0028,701C) | -/1
>>>>>DDL Value | (0028,7017) | -/1
>>>>>Luminance Value | (0028,701F) | -/1
>>>>>CIExy White Point | (0028,7018) | -/3
>>>>Reflected Ambient Light | (2010,0160) | -/3
>>>>Ambient Light Value Source | (0028,7025) | -/1C (Required if Reflected Ambient Light (2010,0160) is present.)

##### EE.2.2.1.2 SCU Behavior

The SCU uses the N-GET to request the SCP to provide the contents of a Display System SOP Instance. The SCU shall specify in the N-GET request primitive the UID of the SOP Instance from which attributes are to be returned.

The SCU shall specify the list of Display System Attributes for which values are to be returned. The SCU shall not specify Attributes which are defined within a Sequence, but rather specify the sequence itself to be returned in its entirety.

The SCU shall specify in the N-GET request primitive the well-known UID of the SOP Instance.

##### EE.2.2.1.3 SCP Behavior

The SCP shall return the values for the specified Attributes of the Display System SOP Instance.

The SCP shall return the status code for the requested SOP Instance retrieval. The meaning of success, warning, and failure status codes are defined in PS3.7.

Prev | Up | Next
EE.2 Display System SOP Class | Home | EE.2.3 SOP Class Definitions and UIDs

DICOM PS3.4 2018a - Service Class Specifications