DICOM PS3.3 2018a - Information Object Definitions

A.17 RT Image IOD
Prev | A Composite Information Object Definitions (Normative) | Next

## A.17 RT Image IOD

### A.17.1 RT Image IOD Description

The focus for this Radiotherapy Image IOD (RT Image IOD) is to address the requirements for image transfer found in general radiotherapy applications performed on conventional simulators, virtual simulators, and portal imaging devices. Such images have a conical imaging geometry and may either be acquired directly from the device, or digitized using a film digitizer. Numeric beam data parameters may also be recorded with the image, indicating the parameter values at the time the image was taken or created.

Prev | Up | Next
A.16.3 XRF Image IOD Module Table | Home | A.17.2 RT Image IOD Entity-Relationship Model

DICOM PS3.3 2018a - Information Object Definitions