DICOM PS3.3 2018a - Information Object Definitions

A.8.3.3 Multi-frame Grayscale Byte SC Image IOD Module Table
Prev | A.8.3 Multi-frame Grayscale Byte Secondary Capture Image IOD | Next

#### A.8.3.3 Multi-frame Grayscale Byte SC Image IOD Module Table

Table A.8-3 specifies the Modules of the Multi-frame Grayscale Byte SC Image IOD.

Table A.8-3. Multi-frame Grayscale Byte SC Image IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Clinical Trial Series | C.7.3.2 | U
Equipment | General Equipment | C.7.5.1 | U
SC Equipment | C.8.6.1 | M
Frame of Reference | Frame of Reference | C.7.4.1 | C - Required if Pixel Measures or Plane Position (Patient) or Plane Orientation (Patient) Functional Group Macros Present
Synchronization | C.7.4.2 | U
Image | General Image | C.7.6.1 | M
General Reference | C.12.4 | U
Image Pixel | C.7.6.3 | M
Cine | C.7.6.5 | C - Required if Frame Increment Pointer (0028,0009) is Frame Time (0018,1063) or Frame Time Vector (0018,1065)
Multi-frame | C.7.6.6 | M
Frame Pointers | C.7.6.9 | U
Device | C.7.6.12 | U
Multi-frame Functional Groups | C.7.6.16 | U
Multi-frame Dimension | C.7.6.17 | U
Specimen | C.7.6.22 | U
SC Image | C.8.6.2 | U
SC Multi-frame Image | C.8.6.3 | M
SC Multi-frame Vector | C.8.6.4 | C - Required if Number of Frames is greater than 1
VOI LUT | C.11.2 | C - Required if the VOI LUT stage is not an identity transformation
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | U
Frame Extraction | C.12.3 | C - Required if the SOP Instance was created in response to a Frame-Level retrieve request

Prev | Up | Next
A.8.3.2 Multi-frame Grayscale Byte SC Image IOD Entity-Relationship Model | Home | A.8.3.4 Multi-frame Grayscale Byte SC Image IOD Content Constraints

DICOM PS3.3 2018a - Information Object Definitions