DICOM PS3.3 2018a - Information Object Definitions

A.34.6.4.5 Sampling Frequency
Prev | A.34.6.4 Hemodynamic IOD Content Constraints | Next

##### A.34.6.4.5 Sampling Frequency

The value of Sampling Frequency (003A,001A) in each Waveform Sequence Item shall be less than or equal to 400.

Prev | Up | Next
A.34.6.4.4 Number of Waveform Channels | Home | A.34.6.4.7 Channel Source

DICOM PS3.3 2018a - Information Object Definitions