DICOM PS3.3 2018a - Information Object Definitions

C.7.6.19 Supplemental Palette Color Lookup Table Module
Prev | C.7.6 Common Image IE Modules | Next

#### C.7.6.19 Supplemental Palette Color Lookup Table Module

This module is used in conjunction with Multi-frame IODs that use RGB color in a number of frames. The value of Pixel Presentation (0008,9205) for such frames equals COLOR.

Table C.7.6.19-1 specifies the Attributes that describe the Lookup table data.

Table C.7.6.19-1. Supplemental Palette Color Lookup Table Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Red Palette Color Lookup Table Descriptor | (0028,1101) | 1 | Specifies the format of the Red Palette Color Lookup Table Data (0028,1201). See Section C.7.6.3.1.5 for further explanation.
Green Palette Color Lookup Table Descriptor | (0028,1102) | 1 | Specifies the format of the Green Palette Color Lookup Table Data (0028,1202). See Section C.7.6.3.1.5 for further explanation.
Blue Palette Color Lookup Table Descriptor | (0028,1103) | 1 | Specifies the format of the Blue Palette Color Lookup table Data (0028,1203). See Section C.7.6.3.1.5 for further explanation.
Red Palette Color Lookup Table Data | (0028,1201) | 1 | Red Palette Color Lookup Table Data. See Section C.7.6.3.1.6 for further explanation.
Green Palette Color Lookup Table Data | (0028,1202) | 1 | Green Palette Color Lookup Table Data. See Section C.7.6.3.1.6 for further explanation.
Blue Palette Color Lookup Table Data | (0028,1203) | 1 | Blue Palette Color Lookup Table Data. See Section C.7.6.3.1.6 for further explanation.

Prev | Up | Next
C.7.6.18.3 Bulk Motion Synchronization Module | Home | C.7.6.20 Patient Orientation Module

DICOM PS3.3 2018a - Information Object Definitions