DICOM PS3.4 2018a - Service Class Specifications

CC.2.7.4 Status Codes
Prev | CC.2.7 Get Unified Procedure Step Information (N-GET) | Next

#### CC.2.7.4 Status Codes

Table CC.2.7-1 defines the status code values that might be returned in a N-GET response. General status code values and fields related to status code values are defined for N-GET DIMSE Service in PS3.7.

Table CC.2.7-1. Status Values

Service Status | Further Meaning | Status Code
--- | --- | ---
Warning | Requested optional Attributes are not supported | 0001
Failure | Failed: Specified SOP Instance UID does not exist or is not a UPS Instance managed by this SCP | C307

Prev | Up | Next
CC.2.7.3 Service Class Provider Behavior | Home | CC.2.8 Search for Unified Procedure Step (C-FIND)

DICOM PS3.4 2018a - Service Class Specifications