DICOM PS3.3 2018a - Information Object Definitions

C.8.30 Corneal Topography Map Modules
Prev | C.8 Modality Specific Modules | Next

### C.8.30 Corneal Topography Map Modules

#### C.8.30.1 Corneal Topography Map Series Module

Table C.8.30.1-1 specifies the Attributes that identify and describe general information about the Corneal Topography Map Series.

Table C.8.30.1-1. Corneal Topography Map Series Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Modality | (0008,0060) | 1 | Type of equipment that created the maps in this Series. Enumerated Values: OPM See Section C.7.3.1.1.1 for further explanation.
Referenced Performed Procedure Step Sequence | (0008,1111) | 1C | Uniquely identifies the Performed Procedure Step SOP Instance to which the Series is related (e.g., a Modality or General-Purpose Performed Procedure Step SOP Instance). Only a single Item shall be included in this Sequence. Required if the Modality Performed Procedure Step SOP Class, or General Purpose Performed Procedure Step SOP Class is supported.
>Include Table 10-11 “SOP Instance Reference Macro Attributes” |
Body Part Examined | (0018,0015) | 1 | Text description of the part of the body examined. Enumerated Values: EYE ### Note Some IODs support the Anatomic Region Sequence (0008,2218), which can provide a more comprehensive mechanism for specifying the body part being examined.

Prev | Up | Next
C.8.29.2 Scan Procedure Module | Home | C.8.30.2 Corneal Topography Map Image Module

DICOM PS3.3 2018a - Information Object Definitions