DICOM PS3.4 2018a - Service Class Specifications

H.4.6.5 Reserved Identifications
Prev | H.4.6 Printer SOP Class | Next

#### H.4.6.5 Reserved Identifications

The well-known UID of the Printer SOP Instance shall have the value "1.2.840.10008.5.1.1.17".

Prev | Up | Next
H.4.6.4 SOP Class Definition and UID | Home | H.4.7 VOI LUT Box SOP Class(Retired)

DICOM PS3.4 2018a - Service Class Specifications