DICOM PS3.17 2018a - Explanatory Information

BBB.3.4 Treatment-delivery With External Verification - Machine Adjustment Required
Prev | BBB.3 Use Cases | Next

### BBB.3.4 Treatment-delivery With External Verification - Machine Adjustment Required

#### BBB.3.4.1 Message Sequencing

Figure BBB.3.4.1-1 illustrates a message sequence example for the external verification model in the case where the Machine Parameter Verifier (MPV) detects that one or more machine adjustments are required before authorizing treatment, and the TDS has been configured to retrieve the failure information and make the required adjustments.

The steps in this use case replace Steps 8a to 9f in Use Case BBB.3.2, for the case where only a single beam is delivered.

Figure BBB.3.4.1-1. Treatment Delivery Message Sequence - Machine Adjustment Required

Prev | Up | Next
BBB.3.3.2 Transactions and Message Flow | Home | BBB.3.4.2 Transactions and Message Flow

DICOM PS3.17 2018a - Explanatory Information