DICOM PS3.3 2018a - Information Object Definitions

A.60.5 Visual Acuity Measurements IOD
Prev | A.60 Ophthalmic Refractive Measurements Information Object Definitions | Next

### A.60.5 Visual Acuity Measurements IOD

#### A.60.5.1 Visual Acuity Measurements IOD Description

The Visual Acuity Measurements IOD is used to capture a patient's visual acuity relative to that of a reference standard patient under given viewing conditions (distance, lighting, etc.).

Prev | Up | Next
A.60.4.3 Subjective Refraction Measurements IOD Module Table | Home | A.60.5.2 Visual Acuity Measurements IOD Entity-Relationship Model

DICOM PS3.3 2018a - Information Object Definitions