DICOM PS3.3 2018a - Information Object Definitions

C.8.8.15.4 Oscillating Source Movement
Prev | C.8.8.15 RT Brachy Application Setups Module | Next

##### C.8.8.15.4 Oscillating Source Movement

In brachytherapy treatment techniques involving oscillating source movement (i.e., when Source Movement Type (300A,0288) is OSCILLATING), the Brachy Control Point Sequence (300A,02D0) shall consist of two items. The first Control Point shall have Cumulative Time Weight (300A,02D6) = 0, and Control Point Relative Position (300A,02D2) equal to one end point of the oscillation. The second Control Point shall have Cumulative Time Weight (300A,02D6) = Final Cumulative Time Weight (300A,02C8), and Control Point Relative Position (300A,02D2) equal to the other end point of the oscillation. Transit time shall not be modeled explicitly for oscillating techniques.

Prev | Up | Next
C.8.8.15.3 Channel Length | Home | C.8.8.15.5 Channel Shields

DICOM PS3.3 2018a - Information Object Definitions