DICOM PS3.16 2018b - Content Mapping Resource

TID 10003B Irradiation Event X-Ray Source Data
Prev | X-Ray Radiation Dose SR IOD Templates | Next

### TID 10003B Irradiation Event X-Ray Source Data

This Template contains data that is expected to be available to the X-Ray source component of the equipment.

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 10003B. Irradiation Event X-Ray Source Data

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | NUM | EV (113738, DCM, "Dose (RP) ") | 1 | MC | IF TID (10001) Row 2 = (113704, DCM, "Projection X-Ray") AND any of the values of TID (10001) Row 18 are not (113858, DCM, "MPPS Content") | UNITS = EV (Gy, UCUM, "Gy")
2 |  |  | TEXT | EV (113780, DCM, "Reference Point Definition") | 1 | MC | IF Row 1 is present and Row 3 is not present |
3 |  |  | CODE | EV (113780, DCM, "Reference Point Definition") | 1 | MC | IF Row 1 is present and Row 2 is not present | DCID 10025 “Radiation Dose Reference Points”
4 |  |  | NUM | EV (111631, DCM, "Average Glandular Dose") | 1 | MC | IFF TID (10001) Row 2 = (P5-40010, SRT, "Mammography") | UNITS = EV (mGy, UCUM, "mGy")
5 |  |  | CODE | EV (113732, DCM, "Fluoro Mode") | 1 | UC | IFF TID (10003) Row 7 value = (P5-06000, SRT, "Fluoroscopy") | DCID 10004 “Fluoro Modes”
6 |  |  | NUM | EV (113791, DCM, "Pulse Rate") | 1 | MC | IFF Row 5 value = (113631, DCM, "Pulsed") | UNITS = EV ({pulse}/s, UCUM, "pulse/s")
7 |  |  | NUM | EV (113768, DCM, "Number of Pulses") | 1 | MC | IFF Row 5 is not present or Row 5 is present and equals (113631, DCM, "Pulsed") | UNITS = EV (1, UCUM, "no units")
8 | > | HAS CONCEPT MOD | CODE | EV (121401, DCM, "Derivation") | 1 | MC | IFF count of pulses in Row 7 is estimated | EV (R-10260, SRT, "Estimated")
9 |  |  | NUM | EV (113793, DCM, "Pulse Width") | 1-n | U |  | UNITS = EV (ms, UCUM, "ms")
10 |  |  | NUM | EV (113742, DCM, "Irradiation Duration") | 1 | U |  | UNITS = EV (s, UCUM, "s")
11 |  |  | NUM | EV (113733, DCM, "KVP") | 1-n | M |  | UNITS = EV (kV, UCUM, "kV")
12 |  |  | NUM | EV (113734, DCM, "X-Ray Tube Current") | 1-n | MC | IF Row 15 is not present | UNITS = EV (mA, UCUM, "mA")
13 |  |  | NUM | EV (113767, DCM, "Average X-Ray Tube Current") | 1 | U |  | UNITS = EV (mA, UCUM, "mA")
14 |  |  | NUM | EV (113824, DCM, "Exposure Time") | 1 | MC | IF Row 15 is not present | UNITS = EV (ms, UCUM, "ms")
15 |  |  | NUM | EV (113736, DCM, "Exposure") | 1-n | MC | IF Row 12 or 14 is not present | UNITS = EV (uA.s, UCUM, "uA.s")
16 |  |  | NUM | EV (113766, DCM, "Focal Spot Size") | 1 | U |  | UNITS = EV (mm, UCUM, "mm")
17 |  |  | CODE | EV (111632, DCM, "Anode Target Material") | 1 | U |  | DCID 10016 “Anode Target Material”
18 |  |  | CONTAINER | EV (113771, DCM, "X-Ray Filters") | 1-n | U |  |
19 | > | CONTAINS | CODE | EV (113772, DCM, "X-Ray Filter Type") | 1 | U |  | DCID 10007 “X-Ray Filter Types”
20 | > | CONTAINS | CODE | EV (113757, DCM, "X-Ray Filter Material") | 1 | U |  | DCID 10006 “X-Ray Filter Materials”
21 | > | CONTAINS | NUM | EV (113758, DCM, "X-Ray Filter Thickness Minimum") | 1 | U |  | UNITS = EV (mm, UCUM, "mm")
22 | > | CONTAINS | NUM | EV (113773, DCM, "X-Ray Filter Thickness Maximum") | 1 | U |  | UNITS = EV (mm, UCUM, "mm")
23 |  |  | NUM | EV (113790, DCM, "Collimated Field Area") | 1 | U |  | UNITS = EV (m2, UCUM, "m2")
24 |  |  | NUM | EV (113788, DCM, "Collimated Field Height") | 1 | U |  | UNITS = EV (mm, UCUM, "mm")
25 |  |  | NUM | EV (113789, DCM, "Collimated Field Width") | 1 | U |  | UNITS = EV (mm, UCUM, "mm")
26 |  |  | CODE | EV (111635, DCM, "X-Ray Grid") | 1-n | U |  | DCID 10017 “X-Ray Grid”
27 |  |  | INCLUDE | DTID 1021 “Device Participant” | 1 | MC | Required if the irradiating device is not the recording device. | $DeviceProcedureRole = EV (113859, DCM, "Irradiating Device")

Content Item Descriptions

Row 1 | Dose applied by this irradiation event, relative to defined reference point.
Row 7 | If a precise count of pulses is not available, an estimated number shall be provided, and the Row 8 Concept Modifier shall indicate "Estimated"
Row 9 | Pulse width as measured/recorded by the system, either as a single total value, or as multiple values. If multiple values are provided, their number shall match the value in Row 7 "Number of Pulses".
Row 11 | KVP value as measured/recorded by system, either as a single mean value, or as multiple values. If multiple values are provided, their number shall match the value in Row 7 "Number of Pulses".
Row 12 | Tube current as measured/recorded by system, either as a single mean value, or as multiple values. If multiple values are provided, their number shall match the value in Row 7 "Number of Pulses".
Row 14 | Exposure time as measured/recorded by the system.
Row 15 | Exposure as measured/recorded by system, either as a single total value, or as multiple values. If multiple values are provided, their number shall match the value in Row 7 "Number of Pulses". The Exposure will be affected by the shape of the pulse and other factors, and may not be a simple multiplication of tube current and exposure time.
Row 18 | If one or more Filter(s) were applied during this irradiation event
Row 23 | Collimated area at the receptor plane.
Row 27 | The device that produced the irradiation in this Irradiation Event. I.e., the X-Ray source. This is not required to be present if the information is the same as that already recorded in TID 1004 “Device Observer Identifying Attributes” encoded via the inclusion of TID 1002 “Observer Context” in TID 10001 “Projection X-Ray Radiation Dose” Row 5, which in turn may be absent if identical to the content in the Enhanced General Equipment Module.

Prev | Up | Next
TID 10003A Irradiation Event X-Ray Detector Data | Home | TID 10003C Irradiation Event X-Ray Mechanical Data

DICOM PS3.16 2018b - Content Mapping Resource