DICOM PS3.3 2018b - Information Object Definitions

A.41.3 Ophthalmic Photography 8 Bit Image IOD Modules
Prev | A.41 Ophthalmic Photography 8 Bit Image IOD | Next

### A.41.3 Ophthalmic Photography 8 Bit Image IOD Modules

Table A.41-1. Ophthalmic Photography 8 Bit Image IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Ophthalmic Photography Series | C.8.17.1 | M
Clinical Trial Series | C.7.3.2 | U
Frame of Reference | Synchronization | C.7.4.2 | M
Equipment | General Equipment | C.7.5.1 | M
Image | General Image | C.7.6.1 | M
General Reference | C.12.4 | U
Image Pixel | C.7.6.3 | M
Enhanced Contrast/Bolus | C.7.6.4b | C - Required if contrast was administered, see Section A.41.4.2
Cine | C.7.6.5 | C - Required if there is a sequential temporal relationship between all frames
Multi-frame | C.7.6.6 | M
Device | C.7.6.12 | U
Acquisition Context | C.7.6.14 | U
Ophthalmic Photography Image | C.8.17.2 | M
Ocular Region Imaged | C.8.17.5 | M
Ophthalmic Photography Acquisition Parameters | C.8.17.4 | M
Ophthalmic Photographic Parameters | C.8.17.3 | M
ICC Profile | C.11.15 | U
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | U
Frame Extraction | C.12.3 | C - Required if the SOP Instance was created in response to a Frame-Level retrieve request

### Note

The Specimen Identification Module was previously included in this IOD but has been retired. See PS3.3-2008.

Prev | Up | Next
A.41.2 Ophthalmic Photography 8 Bit Image IOD Entity-Relationship Model | Home | A.41.4 Ophthalmic Photography 8 Bit Image IOD Content Constraints

DICOM PS3.3 2018b - Information Object Definitions