DICOM PS3.3 2018b - Information Object Definitions

C.29.2 Implant Assembly Template
Prev | C.29 Implant Modules | Next

### C.29.2 Implant Assembly Template

This section describes the specific Modules for the Implant Assembly Template IOD. This IOD references Instances of the Implant Template IOD.

#### C.29.2.1 Implant Assembly Template Module

Table C.29.2-1 defines the general Attributes of the Implant Assembly Template Module.

Table C.29.2-1. Implant Assembly Template Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Effective DateTime | (0068,6226) | 1 | Date and time from which on this Instance is valid.
Implant Assembly Template Name | (0076,0001) | 2 | A name given to the assembly described in this instance.
Implant Assembly Template Issuer | (0076,0003) | 1 | The person or organization who issued the assembly template.
Implant Assembly Template Version | (0076,0006) | 2 | The version code of the Implant Assembly Template.
Replaced Implant Assembly Template Sequence | (0076,0008) | 1C | Reference to the Implant Assembly Template that is replaced by this Instance. Only a single Item shall be included in this Sequence. Required if the Instance replaces another Instance.
>Include Table 10-11 “SOP Instance Reference Macro Attributes” |
Implant Assembly Template Type | (0076,000A) | 1 | Indicates whether the Implant Assembly Template is derived from another Instance. Enumerated Values: ORIGINAL DERIVED
Original Implant Assembly Template Sequence | (0076,000C) | 1C | Reference to the Implant Assembly Template Instance with Implant Assembly Template Type (0076,000A) ORIGINAL from which this Instance was ultimately derived. Only a single Item shall be included in this Sequence. Required if Implant Assembly Template Type (0076,000A) is DERIVED.
>Include Table 10-11 “SOP Instance Reference Macro Attributes” |
Derivation Implant Assembly Template Sequence | (0076,000E) | 1C | Reference to the Implant Template Instance from which this Instance was directly derived. Only a single Item shall be included in this Sequence. Required if Implant Assembly Template Type (0076,000A) is DERIVED.
>Include Table 10-11 “SOP Instance Reference Macro Attributes” |
Implant Assembly Template Target Anatomy Sequence | (0076,0010) | 1 | Identifies the anatomical region the implant assembly is to be implanted to. One or more Items shall be included in this Sequence.
>Anatomic Region Sequence | (0008,2218) | 1 | Sequence that identifies the anatomic region of interest in this Instance (i.e., external anatomy, surface anatomy, or general region of the body). Only a single Item shall be included in this Sequence.
>>Include Table 8.8-1 “Code Sequence Macro Attributes” | Defined CID 7304 “Implant Target Anatomy”.
Procedure Type Code Sequence | (0076,0020) | 1 | Coded description of the procedure by which the assembly is implanted. One or more Items shall be included in this Sequence.
>Include Table 8.8-1 “Code Sequence Macro Attributes” | Baseline CID 7301 “Intervention Types”.
Surgical Technique | (0076,0030) | 3 | The surgical technique associated with this assembly template.
MIME Type of Encapsulated Document | (0042,0012) | 2 | The type of the encapsulated document stream described using the MIME Media Type (see RFC 2046). Enumerated Values: application/pdf
Encapsulated Document | (0042,0011) | 2 | Encapsulated Document stream, containing a document encoded according to the MIME Type. PDF description of the surgical technique.
Component Types Sequence | (0076,0032) | 1 | Sets of components of which the assembly is constructed. One or more Items shall be included in this Sequence.
>Component Type Code Sequence | (0076,0034) | 1 | Label assigned to that type of component. Only a single Item shall be included in this Sequence.
>>Include Table 8.8-1 “Code Sequence Macro Attributes” | Baseline CID 7307 “Implant Component Types”.
>Exclusive Component Type | (0076,0036) | 1 | Indicates that only one component of this Component Type shall be used in an assembly. Defined Terms: YES NO
>Mandatory Component Type | (0076,0038) | 1 | Indicates that at least one component of this Component Type has to be used in an assembly. Defined Terms: YES NO
>Component Sequence | (0076,0040) | 1 | References to implant template components used in the assembly. One or more Items shall be included in this Sequence.
>>Include Table 10-11 “SOP Instance Reference Macro Attributes” |
>>Component ID | (0076,0055) | 1 | Numeric ID of the Implant Template. Uniquely identifies the Implant Template within the SOP instance. The value shall start at 1, and increase monotonically by 1 for each Item.
Component Assembly Sequence | (0076,0060) | 3 | Information about how to connect the implants from the component groups. One or more Items are permitted in this Sequence. See Section C.29.2.1.1.1 for details.
>Component 1 Referenced ID | (0076,0070) | 1 | Value of Component ID (0076,0055) present in Component Sequence (0076,0040) that contains the assembly implant components. The ID selects the first component of the connection.
>Component 1 Referenced Mating Feature Set ID | (0076,0080) | 1 | Value of the Mating Feature Set ID (0068,63C0) present in the Mating Feature Set Sequence (0068,63B0) that contains the Mating Feature Sets. The ID selects the Mating Feature Set of the first component of the connection.
>Component 1 Referenced Mating Feature ID | (0076,0090) | 1 | Value of the Mating Feature ID (0068,63F0) present in the Mating Feature Sequence (0068,63E0) that contains the Mating Features. The ID selects the Mating Feature of the Mating Feature Set of the first component of the connection.
>Component 2 Referenced ID | (0076,00A0) | 1 | Value of Component ID (0076,0055) present in Component Sequence (0076,0040) that contains the assembly implant components. The ID selects the second component of the connection.
>Component 2 Referenced Mating Feature Set ID | (0076,00B0) | 1 | Value of the Mating Feature Set ID (0068,63C0) present in the Mating Feature Set Sequence (0068,63B0) that contains the Mating Feature Sets. The ID selects the Mating Feature Set of the second component of the connection.
>Component 2 Referenced Mating Feature ID | (0076,00C0) | 1 | Value of the Mating Feature ID (0068,63F0) present in the Mating Feature Sequence (0068,63E0) that contains the Mating Features. The ID selects the Mating Feature of the Mating Feature Set of the second component of the connection.

##### C.29.2.1.1 Implant Assembly Template Module Attribute Description

###### C.29.2.1.1.1 Component Assembly Sequence

This Sequence defines a table that establishes relations between Mating Features in Implant Templates. This table contains possible connections for the surgical technique described in an instance.

Prev | Up | Next
C.29 Implant Modules | Home | C.29.3 Implant Template Group Module

DICOM PS3.3 2018b - Information Object Definitions