DICOM PS3.4 2018b - Service Class Specifications

GG Non-Patient Object Storage Service Class
Prev |  | Next

# GG Non-Patient Object Storage Service Class

## GG.1 Overview

### GG.1.1 Scope

The Non-Patient Object Storage Service Class defines an application-level class-of-service that allows one DICOM AE to send a SOP Instance of a non-patient-related information object to another DICOM AE.

### GG.1.2 Service Definition

The Non-Patient Object Storage Service Class includes several SOP Classes, each using an IOD defined in PS3.3 (see Section GG.3). The Non-Patient Object Storage Service Class uses the C-STORE DIMSE Service specified in PS3.7. A successful completion of the C-STORE has the following semantics:

- Both the SCU and the SCP support the type of information to be stored.

- The transferred information is stored in some medium.

- For some time frame, the stored information may be accessed.

### Note

1. Support for the Non-Patient Object Storage Service Class does not imply support for any related Query/Retrieve Service Classes.

2. The duration of the storage is also implementation dependent, but is described in the Conformance Statement of the SCP.

3. The Non-Patient Object Storage Service Class is intended to be used in a variety of environments: e.g., for workstations to transfer SOP Instances to other workstations or archives, for archives to transfer SOP Instances to workstations, etc.

Prev |  | Next
FF.4.2 Conformance Statement For An SCP | Home | GG.2 Association Negotiation

DICOM PS3.4 2018b - Service Class Specifications