DICOM PS3.16 2018b - Content Mapping Resource

TID 4010 Mammography CAD Calcification Cluster
Prev | Mammography CAD SR IOD Templates | Next

### TID 4010 Mammography CAD Calcification Cluster

This Template provides the detail specific to a calcification cluster.

Type:

  Non-Extensible

Order:

  Significant

Root:

  No

Table TID 4010. Mammography CAD Calcification Cluster

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CODE | EV (111009, DCM, "Calcification Type") | 1-n | MC | At least one of rows 1, 2, 3, 4, 5 shall be present | DCID 6010 “Mammography Calcification Types”
2 |  |  | CODE | EV (111008, DCM, "Calcification Distribution") | 1 | MC | At least one of rows 1, 2, 3, 4, 5 shall be present | DCID 6012 “Calcification Distribution Modifier”
3 |  |  | NUM | EV (111038, DCM, "Number of calcifications") | 1 | MC | At least one of rows 1, 2, 3, 4, 5 shall be present | UNITS = EV (1, UCUM, "no units") Value = Integer > = 1
4 |  |  | INCLUDE | DTID 1400 “Linear Measurement” | 1-n | MC | At least one of rows 1, 2, 3, 4, 5 shall be present | If the measured path is encoded, the SCOORD and its by-reference relationship to the IMAGE in TID 1400 “Linear Measurement” shall be used.
5 |  |  | INCLUDE | DTID 1401 “Area Measurement” | 1-n | MC | At least one of rows 1, 2, 3, 4, 5 shall be present | If the measured path is encoded, the SCOORD and its by-reference relationship to the IMAGE in TID 1401 “Area Measurement” shall be used.
6 |  |  | INCLUDE | DTID 1402 “Volume Measurement” | 1-n | U |  | If the measured path is encoded, the SCOORD and its by-reference relationship to the IMAGE in TID 1402 “Volume Measurement” shall be used.

Prev | Up | Next
TID 4009 Mammography CAD Individual Calcification | Home | TID 4011 Mammography CAD Density

DICOM PS3.16 2018b - Content Mapping Resource