DICOM PS3.2 2018b - Conformance

K.4.4 Configuration
Prev | K.4 Networking | Next

### K.4.4 Configuration

#### K.4.4.1 QIDO-RS Interface

The EXAMPLE-QIDO-SERVICE can be configured to respond on one port for TLS protected traffic. The TLS port will refuse any connection from a system that is not recognized as authenticated by a known authority.

Prev | Up | Next
K.4.3.3 IPv4 and IPv6 Support | Home | K.5 Media Interchange

DICOM PS3.2 2018b - Conformance