DICOM PS3.17 2018b - Explanatory Information

JJJ.3 One Single Shot With Texture Acquisition As Mesh
Prev | JJJ Optical Surface Scan | Next

## JJJ.3 One Single Shot With Texture Acquisition As Mesh

Use cases: A scanner device providing triangulated objects with textures, e.g., for documentation of burns or virtual autopsy.

The Surface Scan Mesh instance will be used because a triangulated object is stored. A study with two series will be created. One series contains a Surface Mesh instance and the other series a VL Photographic Image instance. The latter stores the texture, which is mapped on the surface mesh and is linked to the Surface Scan Mesh instance via the UV Mapping Sequence (0080,0008).

Figure JJJ.3-1. One Single Shot With Texture Acquisition As Mesh

Prev | Up | Next
JJJ.2 One Single Shot Without Texture Acquisition As Point Cloud | Home | JJJ.4 Storing Modified Point Cloud With Texture As Mesh

DICOM PS3.17 2018b - Explanatory Information