DICOM PS3.3 2018b - Information Object Definitions

A.83.4 Ophthalmic Optical Coherence Tomography En Face Image Image IOD Content Constraints
Prev | A.83 Ophthalmic Optical Coherence Tomography En Face Image Information Object Definition | Next

### A.83.4 Ophthalmic Optical Coherence Tomography En Face Image Image IOD Content Constraints

The following constraints on Series and Image Attributes take precedence over the descriptions given in the Module Attribute Tables.

#### A.83.4.1 Frame of Reference UID

The value for the Frame of Reference UID (0020,0052) in this SOP Instance shall convey the same value as the Frame of Reference UID (0020,0052) of the SOP Instance(s) referenced in Attribute Source Image Sequence (0008,2112).

Prev | Up | Next
A.83.3 Ophthalmic Optical Coherence Tomography En Face Image IOD Modules | Home | A.84 Ophthalmic Optical Coherence Tomography B-scan Volume Analysis Information Object Definition

DICOM PS3.3 2018b - Information Object Definitions