DICOM PS3.3 2018b - Information Object Definitions

C.8.24.2.2 Ultrasound Frame of Reference Module Attributes
Prev | C.8.24.2 Ultrasound Frame of Reference Module | Next

##### C.8.24.2.2 Ultrasound Frame of Reference Module Attributes

###### C.8.24.2.2.1 Volume to Transducer Mapping Matrix

The Volume to Transducer Mapping Matrix (0020,9309) is used to describe the relationship between the Transducer Frame of Reference coordinate system and the Volume Frame of Reference coordinate system.

The Volume to Transducer Mapping Matrix ([MTV] = [P]*[Q]) describes how to transform a point (XV, YV, ZV) in the Volume coordinate system into (XX,YX, ZX) in the Transducer coordinate system according to the equation below.

Where:

XVYVZV

  The voxel location (in mm) in the Volume Frame of Reference

XXYXZX

  The voxel location (in mm) in the Transducer Frame of Reference

Pij,Pij,Pij

  A 3x3 matrix of direction cosine values as measured to the Transducer origin from the volume origin.

Qx,Qy,Qz

  The translation values (in mm) describe the location in mm of the Transducer Frame of Reference (XX,YX, ZX) origin from the Volume Reference Origin (XV,YV, ZV) measured in millimeters along the Volume axes i.e., to the transducer origin from the volume origin.

###### C.8.24.2.2.2 Volume to Table Mapping Matrix

The Volume to Table Mapping Matrix (0020,930A) is used to describe the relationship between the Volume Frame of Reference coordinate system and a modality specific equipment coordinate system. This mapping can be used only with systems that have a well-defined equipment coordinate system.

The Volume to Table Mapping Matrix([MVG] = [R]*[S]) describes how to transform a point (XVYVZV) in the Volume coordinate system into (XT, YT, ZT) in the Table coordinate system according to the equation below.

Equation C.8.24-1.

Where:

XVYVZV

  The voxel location (in mm) in the Volume Frame of Reference

XTYTZT

  The voxel location (in mm) in the Table Frame of Reference

Rij,Rij,Rij

  A 3x3 matrix of direction cosine values as measured to the gantry origin from the volume origin.

Sx,Sy,Sz

  The translation values (in mm) describe the location in mm of the Table Frame of Reference (XT, YT, ZT) origin from the Volume Reference Origin (XV,YV, ZV) measured in millimeters along the table axes i.e., to the table origin from the volume origin.

### Note

The Mapping Matrices are rigid transformations that involve only translations and rotations. Mathematically, the matrix is orthonormal and describes six degrees of freedom: three translations, and three rotations.

Prev | Up | Next
C.8.24.2 Ultrasound Frame of Reference Module | Home | C.8.24.3 Enhanced US Image Module

DICOM PS3.3 2018b - Information Object Definitions