DICOM PS3.5 2018d - Data Structures and Encoding

A.4.5 MPEG2 Video Compression (Current)
Prev | A.4 Transfer Syntaxes For Encapsulation of Encoded Pixel Data | Next

### A.4.5 MPEG2 Video Compression

The International Standards Organization ISO/IEC MPEG2 has developed an International Standard, [ISO/IEC 13818-2] 'Information Technology - Generic coding of moving pictures and associated audio information: video -- part 2', referred to as "MPEG-2".

A DICOM Transfer Syntax for MPEG2 Video Compression shall be identified by a UID value of either:

- 1.2.840.10008.1.2.4.100 corresponding to MPEG2 Main Profile / Main Level option of the ISO/IEC MPEG2 Video standard

- 1.2.840.10008.1.2.4.101 corresponding to the MPEG2 Main Profile / High Level option of the ISO/IEC MPEG2 Video standard.

Prev | Up | Next
A.4.4 JPEG 2000 Image Compression | Home | A.4.6 MPEG-4 AVC/H.264 High Profile / Level 4.1 Video Compression

DICOM PS3.5 2018d - Data Structures and Encoding