DICOM PS3.4 2018d - Service Class Specifications

CC.2.6 Set Unified Procedure Step Information (N-SET) (Current)
Prev | CC.2 DIMSE Service Groups | Next

### CC.2.6 Set Unified Procedure Step Information (N-SET)

This operation allows an SCU to set Attribute Values of a UPS Instance and provide information about a specific real-world UPS that is under control of the SCU. This operation shall be invoked by the SCU through the DIMSE N-SET Service.

#### CC.2.6.1 Unified Procedure Step IOD Subset Specification

The Application Entity that claims conformance to the UPS Pull SOP Class as an SCU may choose to modify a subset of the Attributes maintained by the SCP. The Application Entity that claims conformance as an SCP to the UPS Pull SOP Class shall support Attributes specified in Table CC.2.5-3

Prev | Up | Next
CC.2.5.4 Status Codes | Home | CC.2.6.2 Service Class User Behavior

DICOM PS3.4 2018d - Service Class Specifications