DICOM PS3.16 2018d - Content Mapping Resource

Mammography CAD SR IOD Templates (Current)
Prev | A Structured Reporting Templates (Normative) | Next

## Mammography CAD SR IOD Templates

The Templates that comprise the Mammography CAD SR IOD are interconnected as in Figure A-8:

Figure A-8. Mammography CAD SR IOD Template Structure

In Figure A-8, '···' indicates possible recursive application of subordinate Templates.

### TID 4000 Mammography CAD Document Root

This Template forms the top of a content tree that allows a mammography CAD device to describe the results of detection and analysis of Mammographic evidence. This Template, together with its subordinate Templates, describes both the results for presentation to radiologists and partial product results for consumption by mammography CAD devices in subsequent mammography CAD reports.

This Template defines a Container that contains an Image Library, the mammography CAD results, and summaries of the detection and analysis algorithms performed. The Image Library contains the Image SOP Class and Instance UIDs, and selected attributes for each image referenced in either the algorithm summaries or mammography CAD results.

The Summary of Detections and Summary of Analyses sub-trees gather lists of algorithms attempted, grouped by success/failure status. Algorithms not attempted are not mentioned in these sub-trees. This information forms the basis for understanding why a mammography CAD report may produce no (or fewer than anticipated) results. Mammography CAD results are constructed bottom-up, starting from Single Image Findings (see TID 4006 “Mammography CAD Single Image Finding”), associated as Composite Features (see TID 4004 “Mammography CAD Composite Feature”), and from which Individual and Overall Impressions are formed.

See Figure E.1-1 “Top Levels of Mammography CAD SR Content Tree” in PS3.17 .

Type:

  Non-Extensible

Order:

  Significant

Root:

  Yes

Table TID 4000. Mammography CAD Document Root

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (111036, DCM, "Mammography CAD Report") | 1 | M |  | Root node
2 | > | HAS CONCEPT MOD | INCLUDE | DTID 1204 “Language of Content Item and Descendants” | 1 | M |  |
3 | > | CONTAINS | CONTAINER | EV (111028, DCM, "Image Library") | 1 | M |  |
4 | >> | CONTAINS | INCLUDE | DTID 4020 “CAD Image Library Entry” | 1-n | M |  | $ImageLaterality = DCID 6022 “Side” $ImageView = DCID 4014 “View for Mammography” $ImageViewMod = DCID 4015 “View Modifier for Mammography”
5 | > | CONTAINS | INCLUDE | DTID 4001 “Mammography CAD Overall Impression/Recommendation” | 1 | M |  |
6 | > | CONTAINS | CODE | EV (111064, DCM, "Summary of Detections") | 1 | M |  | DCID 6042 “Status of Results”
7 | >> | INFERRED FROM | INCLUDE | DTID 4015 “CAD Detections Performed” | 1 | MC | Shall be present unless the value of (111064, DCM, "Summary of Detections") is (111225, DCM, "Not Attempted") | $DetectionCode = DCID 6014 “Mammography Single Image Finding”
8 | > | CONTAINS | CODE | EV (111065, DCM, "Summary of Analyses") | 1 | M |  | DCID 6042 “Status of Results”
9 | >> | INFERRED FROM | INCLUDE | DTID 4016 “CAD Analyses Performed” | 1 | MC | Shall be present unless the value of (111065, DCM, "Summary of Analyses") is (111225, DCM, "Not Attempted") | $AnalysisCode = DCID 6043 “Types of Mammography CAD Analysis”

Content Item Descriptions

Image Library | The "Image Library" section of the Content Tree (TID 4000 “Mammography CAD Document Root”, row 3) shall include all Image SOP Instances from the Current Requested Procedure Evidence Sequence (0040,A375) attribute of the SR Document General module. If a portion of another instance of a Mammography CAD SR IOD is duplicated in the "Overall Impression/ Recommendation" section of the Content Tree, the "Image Library" shall also include all Image Library Entries referenced from the duplicated portions of the Mammography CAD SR.
Detections Performed | The "Detections Performed" and "Analyses Performed" sections of the Content Tree (TID 4000 “Mammography CAD Document Root”, rows 6 and 8) together shall reference all Image SOP Instances included in the Current Requested Procedure Evidence Sequence (0040,A375) attribute of the SR Document General module.
Analyses Performed

Prev | Up | Next
TID 3990 Two Dimensional Measurement Graph | Home | TID 4001 Mammography CAD Overall Impression/Recommendation

DICOM PS3.16 2018d - Content Mapping Resource