DICOM PS3.5 2018d - Data Structures and Encoding

A.4.2 RLE Image Compression (Current)
Prev | A.4 Transfer Syntaxes For Encapsulation of Encoded Pixel Data | Next

### A.4.2 RLE Image Compression

Annex G defines a RLE Image Compression Transfer Syntax. This transfer Syntax is identified by the UID value "1.2.840.10008.1.2.5". If the object allows multi-frame images in the pixel data field, then each frame shall be encoded separately. Each frame shall be encoded in one and only one Fragment (see Section 8.2).

Prev | Up | Next
A.4 Transfer Syntaxes For Encapsulation of Encoded Pixel Data | Home | A.4.3 JPEG-LS Image Compression

DICOM PS3.5 2018d - Data Structures and Encoding