DICOM PS3.3 2018d - Information Object Definitions

C.8.9.3 PET Multi-gated Acquisition Module (Current)
Prev | C.8.9 PET Information Module Definitions | Next

#### C.8.9.3 PET Multi-gated Acquisition Module

Table C.8-62 contains IOD Attributes that describe a PET Multi-gated Acquisition.

Table C.8-62. PET Multi-Gated Acquisition Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Beat Rejection Flag | (0018,1080) | 2 | Heart beat duration sorting has been applied. Enumerated Values: Y yes N no
Trigger Source or Type | (0018,1061) | 3 | Text indicating trigger source. Defined Terms: EKG
PVC Rejection | (0018,1085) | 3 | Description of the type of PVC rejection criteria used.
Skip Beats | (0018,1086) | 3 | Number of beats skipped after a detected arrhythmia.
Heart Rate | (0018,1088) | 3 | Average number of heart beats per minute for the collection period for this image. This shall include all accepted beats as well as rejected beats.
Cardiac Framing Type | (0018,1064) | 3 | Description of type of framing performed. See Section C.7.6.18.1.1.1 for description and Defined Terms.

Prev | Up | Next
C.8.9.2 PET Isotope Module | Home | C.8.9.4 PET Image Module

DICOM PS3.3 2018d - Information Object Definitions