DICOM PS3.3 2018d - Information Object Definitions

A.84 Ophthalmic Optical Coherence Tomography B-scan Volume Analysis Information Object Definition (Current)
Prev | A Composite Information Object Definitions (Normative) | Next

## A.84 Ophthalmic Optical Coherence Tomography B-scan Volume Analysis Information Object Definition

This Section defines an Information Object to be used for multi-frame images obtained from the volumetric analysis of ophthalmic tomography B-scans (e.g., ophthalmic tomography angiographic (blood flow) volume information).

### A.84.1 Ophthalmic Optical Coherence Tomography B-scan Volume Analysis IOD Description

The Ophthalmic Optical Coherence Tomography B-scan Volume Analysis IOD specifies a multi-frame image conveying ophthalmic optical coherence tomography volumetric B-scan volume analysis information (e.g., angiographic (blood flow) volume information).

Prev | Up | Next
A.83.4 Ophthalmic Optical Coherence Tomography En Face Image Image IOD Content Constraints | Home | A.84.2 Ophthalmic Optical Coherence Tomography B-scan Volume Analysis IOD Entity-Relationship Model

DICOM PS3.3 2018d - Information Object Definitions