DICOM PS3.18 2018d - Web Services

8.2.9.2 Unique Identifier of the Series Containing the Presentation SOP Instance (Current)
Prev | 8.2.9 Unique Identifiers of the Presentation State Object | Next

#### 8.2.9.2 Unique Identifier of the Series Containing the Presentation SOP Instance

The parameter name shall be "presentationSeriesUID" for URI mode.

The value is the Series Instance UID of the Series containing the Presentation State storage object to be applied on the images.

If this parameter is present, then the Region of the Image parameter shall not be present. See Section 8.2.4.

The value shall be encoded as a unique identifier (UID) string, as specified in PS3.5, except that it shall not be padded to an even length with a NULL character.

### Note

As specified in DICOM, the Presentation State will be in the same study as the images it applies to.

Prev | Up | Next
8.2.9 Unique Identifiers of the Presentation State Object | Home | 8.2.10 Reserved

DICOM PS3.18 2018d - Web Services