DICOM PS3.3 2018d - Information Object Definitions

C.8.19.5 X-Ray Detector Module (Current)
Prev | C.8.19 Enhanced XA/XRF Image | Next

#### C.8.19.5 X-Ray Detector Module

Table C.8.19.5-1 contains IOD Attributes that describe an X-Ray detector.

Table C.8.19.5-1. X-Ray Detector Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Include Table C.8-71b “Digital X-Ray Detector Macro Attributes” |
Physical Detector Size | (0018,9429) | 1 | Dimensions of the physical detector measured in mm as a row size followed by a column size.
Position of Isocenter Projection | (0018,9430) | 1C | Position of the Isocenter projection on the detector plane measured in fractional physical detector elements as a distance along the column direction followed by a distance along the row direction from the center of the TLHC detector element of a rectangle circumscribing the physical detector area. Required if Isocenter Reference System Sequence (0018,9462) is present.

Prev | Up | Next
C.8.19.4 X-Ray Image Intensifier Module | Home | C.8.19.6 Enhanced XA/XRF Image Functional Group Macros

DICOM PS3.3 2018d - Information Object Definitions