DICOM PS3.16 2018d - Content Mapping Resource

CID 7250 Multi-Frame Subset Type (Current)
Prev | B DCMR Context Groups (Normative) | Next

## CID 7250 Multi-Frame Subset Type

This Context Group specifies the terms used to identify a subset of frames of a multi-frame image. It is used for encoding an equivalent of the Image SOP Instance Reference Macro (see PS3.3) in an HL7 v3 data structure (see HL7 v3 CMET, COCT_RM830120 "A_DicomCompositeObjectReference minimal").

Resources:

  HTML | FHIR JSON | FHIR XML | IHE SVS XML

Type:

  Extensible

Version:

  20070625

UID:

  1.2.840.10008.6.1.513

Table CID 7250. Multi-Frame Subset Type

Coding Scheme Designator | Code Value | Code Meaning
--- | --- | ---
DCM | 121190 | Referenced Frames
DCM | 121191 | Referenced Segment

Prev | Up | Next
CID 7222 Parametric Map Derivation Image Purpose of Reference | Home | CID 7260 Diffusion Acquisition Value Types

DICOM PS3.16 2018d - Content Mapping Resource