DICOM PS3.17 2018d - Explanatory Information

XXX.3.6.3.2 Volumetric Presentation State Cropping Module Recommendations (Current)
Prev | XXX.3.6.3 Encoding Details | Next

##### XXX.3.6.3.2 Volumetric Presentation State Cropping Module Recommendations

Table XXX.3.6-2. Volumetric Presentation State Cropping Module Recommendations

Attribute Name | Tag | Comment
--- | --- | ---
Volume Cropping Sequence | (0070,1301) | The sequence contains three items, one for each segmented nodule type. For brevity only the first item of the sequence is shown in this table.
>Volume Cropping Method | (0070,1302) | Set to "INCLUDE_SEG"
> Referenced Image Sequence | (0008,1140) | Set references to segments depicting the areas that make up the nodules marked by the segmentation.
>>Referenced SOP Class UID | (0008,1150) | Set to "1.2.840.10008.​5.​1.​4.​1.​1.​66.​4" (Segmentation Storage SOP Class UID)
>>Referenced SOP Instance UID | (0008,1155) | Set to the SOP Instance UID of the instance that contains the Segmentation.
>>Referenced Segment Number | (0062,000B) | Set to the identifier of the relevant segment within the Segmentation instance (e.g., "Large Nodules").
… |  |

Prev | Up | Next
XXX.3.6.3 Encoding Details | Home | XXX.3.6.3.3 Volumetric Presentation State Display Module Recommendations

DICOM PS3.17 2018d - Explanatory Information