DICOM PS3.7 2018d - Message Exchange

C.5.11 Invalid Attribute Value (Current)
Prev | C.5 Failure Status Class | Next

### C.5.11 Invalid Attribute Value

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0106H.
Modification List/Attribute List | (no tag) | - | - | Optionally contains the application specific Data Set to only encode the invalid Attribute Values conveyed in the Modification List of the N-SET -RQ or the Attribute List of the N-CREATE-RQ.

Prev | Up | Next
C.5.10 Invalid Argument Value | Home | C.5.12 Invalid Object Instance

DICOM PS3.7 2018d - Message Exchange