DICOM PS3.3 2018d - Information Object Definitions

C.11.20 XA/XRF Presentation State Shutter Module (Current)
Prev | C.11 Look Up Tables and Presentation States | Next

### C.11.20 XA/XRF Presentation State Shutter Module

Table C.11.19-1 specifies the Attributes that describe shutter operations for a XA/XRF Multi-frame image.

Table C.11.20-1. XA/XRF Presentation State Shutter Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Frame Display Shutter Sequence | (0018,9472) | 1 | Sequence of shutter specifications to be applied to groups of frames. One or more Items shall be included in this Sequence.
>Referenced Image Sequence | (0008,1140) | 1C | Sequence of Items where each Item provides reference to a selected set of Image SOP Class/SOP Instance pairs that are defined in the Presentation State Relationship Module. One or more Items shall be included in this Sequence. Required if shutters in this Item do not apply to all the images and frames listed in the Presentation State Relationship Module.
>>Include Table 10-3 “Image SOP Instance Reference Macro Attributes” |
>Include Table C.7-17a “Display Shutter Macro Attributes” |

Prev | Up | Next
C.11.19 XA/XRF Presentation State Mask Module | Home | C.11.21 XA/XRF Presentation State Presentation Module

DICOM PS3.3 2018d - Information Object Definitions