DICOM PS3.4 2018d - Service Class Specifications

S.3.2.3.3 Service Class Provider Behavior (Current)
Prev | S.3.2.3 Cancel Media Creation | Next

##### S.3.2.3.3 Service Class Provider Behavior

Upon receipt of the N-ACTION Cancel Media Creation request, the SCP shall return, via the N-ACTION response primitive, the N-ACTION Response Status Code applicable to the associated request. A success status conveys that the SCP has successfully canceled the request.

A failure status conveys that the SCP has failed to cancel the request, in which case the Execution Status (2100,0020), Execution Status Info (2100,0030), Total Number of Pieces of Media Created (2200,000B), Failed SOP Sequence (0008,1198) and Referenced Storage Media Sequence (2200,000D) Attributes may subsequently be retrieved by an N-GET.

Prev | Up | Next
S.3.2.3.2 Service Class User Behavior | Home | S.3.2.3.4 Status Codes

DICOM PS3.4 2018d - Service Class Specifications