DICOM PS3.16 2018d - Content Mapping Resource

TID 3303 Stress Test Phase Data (Current)
Prev | Stress Testing Report Templates | Next

### TID 3303 Stress Test Phase Data

The Stress Test Phase Data Template provides a structure for measurements acquired during a single procedure phase.

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 3303. Stress Test Phase Data

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | DT (121070, DCM, "Findings") | 1 | M |  |
2 | > | HAS ACQ CONTEXT | CODE | EV (G-7292, SRT, "Procedure phase") | 1 | MC | XOR row 3 | BCID 3207 “Stress Test Procedure Phases”
3 | > | HAS ACQ CONTEXT | CODE | EV (G-7292, SRT, "Procedure phase") | 1 | MC | IFF Nuclear Imaging; XOR row 2 | DCID 3101 “Cardiac Procedural State Values”
4 | > | HAS ACQ CONTEXT | TEXT | EV (G-7292, SRT, "Procedure phase") | 1 | U |  |
5 | > | CONTAINS | INCLUDE | DTID 3301 “Stress Test Procedure Description” | 1 | MC | IFF protocol changed from initial specification |
6 | > | HAS ACQ CONTEXT | NUM | EV (109055, DCM, "Protocol Stage") | 1 | U |  | UNITS = DT ({stage}, UCUM, "stage")
7 | > | CONTAINS | INCLUDE | DTID 3304 “Stress Test Measurement Group” | 1-n | U |  |
8 | > | CONTAINS | INCLUDE | DTID 3307 “NM/PET Perfusion Measurement Group” | 1 | MC | IFF Nuclear or PET Imaging |
9 | > | CONTAINS | INCLUDE | DTID 3309 “Stress Echo Measurement Group” | 1 | UC | IFF Echocardiography Imaging |

Content Item Descriptions

Row 1 | The Container shall have a specific Content Item Observation DateTime (0040,A032) attribute to indicate the time at which the phase began.

Prev | Up | Next
TID 3301 Stress Test Procedure Description | Home | TID 3304 Stress Test Measurement Group

DICOM PS3.16 2018d - Content Mapping Resource