DICOM PS3.17 2018d - Explanatory Information

XXX.3.6.3.3 Volumetric Presentation State Display Module Recommendations (Current)
Prev | XXX.3.6.3 Encoding Details | Next

##### XXX.3.6.3.3 Volumetric Presentation State Display Module Recommendations

Table XXX.3.6-3. Volumetric Presentation State Display Module Recommendations

Attribute Name | Tag | Comment
--- | --- | ---
Pixel Presentation | (0008,9205) | Set to "TRUE_COLOR"
Presentation State Classification Component Sequence | (0070,1801) | Include four items, one for each classification component.
>ITEM 1
>Component Type | (0070,1802) | Set to "ONE_TO_RGBA"
>Component Input Sequence | (0070,1803) | Set only one item in this sequence since the component has only one input.
>>Input Set Index | (0070,1804) | Set to "1" for the anatomy view.
>RGB LUT Transfer Function | (0028,140F) | Set to "EQUAL_RGB" to map to grayscale RGB values.
>Alpha LUT Transfer Function | (0028,1410) | Set to "NONE". The anatomy is completely opaque.
>ITEM 2
>Component Type | (0070,1802) | Set to "ONE_TO_RGBA"
>Component Input Sequence | (0070,1803) | Set only one item in this sequence since the component has only one input.
>>Input Set Index | (0070,1804) | Set to "2" for the large nodules segmentation.
>RGB LUT Transfer Function | (0028,140F) | Set to "TABLE" to be able to map to "red" colors.
>Alpha LUT Transfer Function | (0028,1410) | Set to "TABLE" to be able to set a transparency for the segmentation.
… |  | Definitions of lookup tables left out for brevity.
>ITEM 3
>Component Type | (0070,1802) | Set to "ONE_TO_RGBA"
>Component Input Sequence | (0070,1803) | Set only one item in this sequence since the component has only one input.
>>Input Set Index | (0070,1804) | Set to "3" for the large nodules segmentation.
>RGB LUT Transfer Function | (0028,140F) | Set to "TABLE" to be able to map to "yellow" colors.
>Alpha LUT Transfer Function | (0028,1410) | Set to "TABLE" to be able to set a transparency for the segmentation.
… |  | Definitions of lookup tables left out for brevity.
>ITEM 4
>Component Type | (0070,1802) | Set to "ONE_TO_RGBA"
>Component Input Sequence | (0070,1803) | Set only one item in this sequence since the component has only one input.
>>Input Set Index | (0070,1804) | Set to "4" for the small nodules segmentation.
>RGB LUT Transfer Function | (0028,140F) | Set to "TABLE" to be able to map to "green" colors.
>Alpha LUT Transfer Function | (0028,1410) | Set to "TABLE" to be able to set a transparency for the segmentation.
… |  | Definitions of lookup tables left out for brevity.
Presentation State Compositor Component Sequence | (0070,1805) | Include three items that define the chain of RGB Compositor components.
>ITEM 1
>Weighting Transfer Function Sequence | (0070,1806) | Contains the two Weighting LUTs from Section XXX.5.2 to create the "Partially Transparent A over B" composting from two RGBA inputs.
… |  | Definitions of lookup tables left out for brevity.
>ITEM 2
>Weighting Transfer Function Sequence | (0070,1806) | Contains the two Weighting LUTs from Section XXX.5.3 to create the "A over B" composting from one RGB and one RGBA input.
… |  | Definitions of lookup tables left out for brevity.
>ITEM 3
>Weighting Transfer Function Sequence | (0070,1806) | Contains the two Weighting LUTs from Section XXX.5.3 to create the "A over B" composting from one RGB and one RGBA input.
… |  | Definitions of lookup tables left out for brevity.
ICC Profile | (0028,2000) | Set to an ICC Profile describing the transformation of the resulting RGB image into PCS-Values.

Prev | Up | Next
XXX.3.6.3.2 Volumetric Presentation State Cropping Module Recommendations | Home | XXX.3.7 Ultrasound Color Flow MPR

DICOM PS3.17 2018d - Explanatory Information