DICOM PS3.16 2018d - Content Mapping Resource

TID 4002 Mammography CAD Impression/Recommendation Body (Current)
Prev | Mammography CAD SR IOD Templates | Next

### TID 4002 Mammography CAD Impression/Recommendation Body

The details of an impression and recommendation are expressed in this Template. It is applied to both Mammography CAD Overall Impression/Recommendation (TID 4001 “Mammography CAD Overall Impression/Recommendation”) and Mammography CAD Individual Impression/Recommendation (TID 4003 “Mammography CAD Individual Impression/Recommendation”).

Type:

  Non-Extensible

Order:

  Significant

Root:

  No

Table TID 4002. Mammography CAD Impression/Recommendation Body

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CODE | EV (111005, DCM, "Assessment Category") | 1-n | MC | At least one of rows 1, 3, 5, 6, 8, 9 shall be present. | DCID 6026 “Mammography Assessment”
2 | > | HAS CONCEPT MOD | CODE | EV (G-C171, SRT, "Laterality") | 1 | U |  | DCID 6022 “Side”
3 |  |  | CODE | EV (111023, DCM, "Differential Diagnosis/ Impression") | 1-n | MC | At least one of rows 1, 3, 5, 6, 8, 9 shall be present. | DCID 6002 “Change Since Last Mammogram or Prior Surgery”
4 | > | HAS CONCEPT MOD | CODE | EV (G-C171, SRT, "Laterality") | 1 | U |  | DCID 6022 “Side”
5 |  |  | TEXT | EV (111033, DCM, "Impression Description") | 1 | MC | At least one of rows 1, 3, 5, 6, 8, 9 shall be present. |
6 |  |  | CODE | EV (111053, DCM, "Recommended Follow-up") | 1-n | MC | At least one of rows 1, 3, 5, 6, 8, 9 shall be present. | DCID 6028 “Mammography Recommended Follow-up”
7 | > | HAS CONCEPT MOD | CODE | EV (G-C171, SRT, "Laterality") | 1 | U |  | DCID 6022 “Side”
8 |  |  | NUM | EV (111055, DCM, "Recommended Follow-up Interval") | 1 | MC | At least one of rows 1, 3, 5, 6, 8, 9 shall be present. May be present only if (111054, DCM, "Recommended Follow-up Date") is not present. | UNITS = DCID 6046 “Units of Follow-up Interval” Values = Integer ≥ 0, where 0 = immediate follow-up
9 |  |  | DATE | EV (111054, DCM, "Recommended Follow-up Date") | 1 | MC | At least one of rows 1, 3, 5, 6, 8, 9 shall be present. May be present only if (111055, DCM, "Recommended Follow-up Interval") is not present. | Shall be later than date of exam
10 |  |  | NUM | EV (111013, DCM, "Certainty of impression") | 1 | UC | May be present only if (111005, DCM, "Assessment Category"), (111023, DCM, "Differential Diagnosis/Impression") or (111033, DCM, "Impression Description") is present. | UNITS = EV (%, UCUM, "Percent") Values = 0 - 100
11 |  |  | INCLUDE | DTID 4019 “Algorithm Identification” | 1-n | M |  |
12 |  |  | NUM | DCID 6142 “Calculated Value” | 1-n | U |  |
13 | > | HAS CONCEPT MOD | CODE | EV (G-C171, SRT, "Laterality") | 1 | U |  | DCID 6022 “Side”
14 | > | HAS CONCEPT MOD | CODE | EV (121401, DCM, "Derivation") | 1 | M |  | DCID 6140 “Calculation Methods”
15 | > | INFERRED FROM | TEXT | EV (112034, DCM, "Calculation Description") | 1 | U |  |

Content Item Descriptions

Certainty of Impression | The certainty that the device populating the Mammography CAD SR report places on this impression, where 0 equals no certainty and 100 equals certainty.
Impression Description | Free-form text describing the overall or an individual impression

Prev | Up | Next
TID 4001 Mammography CAD Overall Impression/Recommendation | Home | TID 4003 Mammography CAD Individual Impression/Recommendation

DICOM PS3.16 2018d - Content Mapping Resource