DICOM PS3.14 2018d - Grayscale Standard Display Function

D.3.2 Application of the Grayscale Standard Display Function (Current)
Prev | D.3 Reflective Display Systems | Next

### D.3.2 Application of the Grayscale Standard Display Function

This last example illustrates how conformance with the Grayscale Standard Display Function may be achieved for a thermal-dye-transfer paper printer/office-light system. The thermal-dye-transfer printer produces black-and-white grayscale prints on a semi-glossy 8-inch x 10-inch heavy-gauge paper. The print is illuminated uniformly by fluorescent lamps so that the minimum reflective density produces a Luminance of 150 cd/m2. The hypothetical transformation operator is assumed to have equal input and output digitization resolution of 8 bits.

Prev | Up | Next
D.3 Reflective Display Systems | Home | D.3.3 Implementation of the Grayscale Standard Display Function

DICOM PS3.14 2018d - Grayscale Standard Display Function