DICOM PS3.17 2018d - Explanatory Information

XXX.3.11.3 Encoding Details (Current)
Prev | XXX.3.11 Colorized Volume Rendering of Segmented Volume Data | Next

#### XXX.3.11.3 Encoding Details

##### XXX.3.11.3.1 Volumetric Presentation State Relationship Module Recommendations

Table XXX.3.11.3.1-1. Volumetric Presentation State Relationship Module Recommendations

Attribute Name | Tag | Comment
Volumetric Presentation Input Set Sequence | (0070,120A) | One item in this sequence
Item #1
>Volumetric Presentation Input Set UID | (0070,1209) | Set to UID1
>Presentation Input Type | (0070,1202) | Set to VOLUME
>Referenced Image Sequence | (0070,1140) | Set reference(s) to the image(s) that make up the input volume
Volumetric Presentation State Input Sequence | (0070, 1201) | Three items are this sequence.
Item #1
>Volumetric Presentation Input Number | (0070,1207) | Set to 1
>Volumetric Presentation Input Set UID | (0070,1209) | Set to UID1
>Include VOI LUT Macro Table C.11-2B | Set to identity
>Crop | (0070, 1204) | Set to 'NO'
>Item #2
>Volumetric Presentation Input Number | (0070,1207) | Set to 2
>Volumetric Presentation Input Set UID | (0070,1209) | Set to UID1
>Include VOI LUT Macro Table C.11-2B | Set to identity
>Crop | (0070, 1204) | Set to 'NO'
>Item #3
>Volumetric Presentation Input Number | (0070,1207) | Set to 3
>Volumetric Presentation Input Set UID | (0070,1209) | Set to UID1
>Include VOI LUT Macro Table C.11-2B | Set to identity
>Crop | (0070, 1204) | Set to 'NO'

Prev | Up | Next
XXX.3.11.2 Encoding Outline | Home | XXX.3.11.3.2 Volume Render Geometry Module Recommendations

DICOM PS3.17 2018d - Explanatory Information