DICOM PS3.3 2018d - Information Object Definitions

A.6.4 US Image IOD Module Table (Current)
Prev | A.6 Ultrasound Image IOD | Next

### A.6.4 US Image IOD Module Table

Table A.6-1 specifies the Modules of the US Image IOD.

Table A.6-1. US Image IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Clinical Trial Series | C.7.3.2 | U
Frame of Reference | Frame of Reference | C.7.4.1 | U
Synchronization | C.7.4.2 | U
Equipment | General Equipment | C.7.5.1 | M
Image | General Image | C.7.6.1 | M
General Reference | C.12.4 | U
Image Pixel | C.7.6.3 | M
Contrast/Bolus | C.7.6.4 | C - Required if contrast media was used in this image
Palette Color Lookup Table | C.7.9 | C - Required if Photometric Interpretation (0028,0004) has a value of PALETTE COLOR
Device | C.7.6.12 | U
Specimen | C.7.6.22 | U
US Region Calibration | C.8.5.5 | U
US Image | C.8.5.6 | M
Overlay Plane | C.9.2 | U
VOI LUT | C.11.2 | U
ICC Profile | C.11.15 | U
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | U

### Note

1. For the purpose of conveying ultrasound protocol data management information it is recommended that the Performed Protocol Code Sequence (0040,0260) be assigned the code value(s) of the performed ultrasound protocol, if any. The Baseline Context Group for these code values is CID 12001 “Ultrasound Protocol Types”.

2. The US Frame of Reference Module was previously included in this IOD, but has been retired. See PS3.3-2003.

#### A.6.4.1 Mutually Exclusive IEs

### Note

A Curve IE was previously included in this IOD that was mutually exclusive with the Image IE, but has been retired. See PS3.3-2004.

Prev | Up | Next
A.6.3 US Image IOD Module Table (Retired) | Home | A.7 Ultrasound Multi-frame Image IOD

DICOM PS3.3 2018d - Information Object Definitions